LABCENTER PROTEUS TOOL INFORMATION FILE
=======================================

In case of difficulty, please e-mail support@labcenter.co.uk

Tool set up for Proteus layout 'filtre.LYT'.
CADCAM generated at 5:49:01 PM on September-06-25.

File List
---------
Top Copper              : filtre - CADCAM Top Copper.TXT
Bottom Copper           : filtre - CADCAM Bottom Copper.TXT
Top Silk Screen         : filtre - CADCAM Top Silk Screen.TXT
Bottom Silk Screen      : filtre - CADCAM Bottom Silk Screen.TXT
Top Solder Resist       : filtre - CADCAM Top Solder Resist.TXT
Bottom Solder Resist    : filtre - CADCAM Bottom Solder Resist.TXT
Top SMT Paste Mask      : filtre - CADCAM Top SMT Paste Mask.TXT
Bottom SMT Paste Mask   : filtre - CADCAM Bottom SMT Paste Mask.TXT
Mechanical 1            : filtre - CADCAM Mechanical 1.TXT
Drill                   : filtre - CADCAM Drill.TXT

Photoplotter Setup
------------------
Format: RS274X, ASCII, 2.4, imperial, absolute, eob=*, LZO
Notes:  D=Diameter, S=Side, W=Width, H=Height, C=Chamfer

D10	CIRCLE  D=40th                                                            DRAW
D11	CIRCLE  D=2.5th                                                           DRAW
D12	CIRCLE  D=10th                                                            DRAW
D13	CIRCLE  D=100th                                                           FLASH
D14	RECT    W=60th                H=200th                                     FLASH
D15	RECT    W=40th                H=60th                                      FLASH
D16	CIRCLE  D=90th                                                            FLASH
D17	CIRCLE  D=8th                                                             DRAW
D18	CIRCLE  D=120th                                                           FLASH
D19	RECT    W=160th               H=300th                                     FLASH
D70	RECT    W=60th                H=80th                                      FLASH
D71	CIRCLE  D=110th                                                           FLASH

NC Drill Setup
--------------
Format: ASCII, 2.4, imperial, absolute, eob=<CR><LF>, no zero suppression.
Notes:  Tool sizes are diameters. Layer sets are in brackets - 0=TOP, 15=BOTTOM, 1-14=INNER.

T01	31.4th (0-15)
T02	40th (0-15)


[END OF FILE]
