#-------------------------------#
# Hardware depending settings
#-------------------------------#
# pin: 255=disabled; x=button x+128=touch button
#button_pin=130
#button2_pin=142
# No specification in config file: try autodetection (gpio4 pin level at startup)
#button_pin=0
#button2_pin=255
#button2_axp=0
# LED port
#led_pout=-1
# OLED Setup is depending on hardware of LoRa board
# TTGO v1:  SDA=4  SCL=15, RST=16 
# TTGO v2:  SDA=21 SCL=22, RST=16
# T-BEAM, OLED: SDA=21, SCL=22, RST=16
# T-BEAM, ILI9225: SDA=4, CLK=21, RS=2, RST=22, CS=0
# No specification in config file: try autodetection (gpio4 pin level at startup)
#
# disptype: 0=OLED, 1=ILI9225
#disptype=0
#oled_sda=21
#oled_scl=22
#oled_rst=16
rxlat=
rxlon=
rxalt=
oled_orient=1
#gps_rxd=-1
#gps_txd=-1
# Frequency correction, in Hz
# freqofs=0
#-------------------------------#
# General config settings
#-------------------------------#
maxsonde=20
debug=0
# wifi mode: 1=client in background; 2=AP in background; 3=client on startup, ap if failure
wifi=3
# TCP/IP KISS TNC in port 14590 for APRSdroid (0=disabled, 1=enabled)
kisstnc.active = 1

# which screens file to use (0: automated selection based on display type and orientation, i>0: screens${i}.txt
# predefined: 1: for OLED, 2: for ILI9225; 3: for ILI9225 (portrait mode); 4: for ILI9431; 5: for ILI9431 (portrait mode)
# screenfile=2
# display configuration. List of "displays"
# first entry: "Scanner" display
# second entry: default "Receiver" display
# additional entries: alternative receiver display, activated by button
display=0,1,2,3,4,5,6,7
# turn off display: 0=never, 1=always, 2=if no RX; (+n*10: after n seconds)
dispsaver=0
# set OLED contrast (0..255) or leave at factory default (-1)
dispcontrast=-1
# set to -1 to disable (used for "N" values in timers in screens.txt). Value in seconds
norx_timeout=20
#Add F4IYT
buzzerOn=1
buzzerPort=25
buzzerFreq=700
dbsmetre=1
#-------------------------------#
# Spectrum display settings
#-------------------------------#
startfreq=400
channelbw=10
spectrum=-1 #10
noisefloor=-125
marker=1
#-------------------------------#
# APRS settings
#-------------------------------#
call=N0CALL
passcode=12345
#-------------------------------#
# Sonde specific settings: bandwidth
# valid values: 3100, 3900, 5200, 6300, 7800, 10400, 12500,
# 15600, 20800, 25000, ...
# other values will be rounded up to the next valid value
# rs92.alt2d: default altitude used by RS92 decoder if only 3 sats available
#-------------------------------#
rs41.agcbw=12500
rs41.rxbw=6300
rs92.rxbw=12500
rs92.alt2d=480
dfm.agcbw=20800
dfm.rxbw=10400
#-------------------------------#
# ftp server for RINEX data (for RS92)
# YYYY/DDD/brdcDDD0.YYn.gz is appended
# s1: igs.bkg.bund.de/IGS/BRDC/
# s2: www.ngs.noaa.gov/cors/rinex/
#-------------------------------#
#ephftp=www.ngs.noaa.gov/cors/rinex/
#ephftp=igs.bkg.bund.de/IGS/BRDC/
ephftp=gssc.esa.int/gnss/data/daily/
#-------------------------------#
# axudp for sending to aprsmap
#-------------------------------#
# local use only, do not feed to public services
# data not sanitized / quality checked, outliers not filtered out
axudp.active=1
axudp.host=192.168.42.20
axudp.port=9002
axudp.symbol=/O
axudp.highrate=1
#-------------------------------#
# connect to some aprs server
#-------------------------------#
tcp.active=0
tcp.host=radiosondy.info
tcp.port=14590
tcp.symbol=/O
tcp.highrate=20
# send beacon (possibly with different call or SSID)
tcp.chase=0
tcp.objcall=
tcp.beaconsym=/`/(
tcp.comment=
#-------------------------------#
# mqtt settings
#-------------------------------#
# data not sanitized / quality checked, outliers not filtered out
mqtt.active=0
mqtt.id=rdz_sonde_server
mqtt.ip=192.168.1.5
mqtt.port=1883
mqtt.username=
mqtt.password=
mqtt.prefix=rdz_sonde_server/
#-------------------------------#
# Sondehub v2 settings
#-------------------------------#
# Sondehub v2 DB settings
sondehub.active=0
sondehub.chase=3
sondehub.host=api.v2.sondehub.org
sondehub.callsign=CHANGEME_RDZTTGO
sondehub.antenna=
sondehub.email=
#-------------------------------#
# Sondehub freq import settings
#-------------------------------#
shfimp.active=0
shfimp.interval=60
shfimp.maxdist=150
shfimp.maxage=6
#-------------------------------#
# EOF
#-------------------------------#
